
**** 02/15/10 16:26:33 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\gerilimbolucu\gerilimbolucu-SCHEMATIC1-sim.sim


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "gerilimbolucu-SCHEMATIC1-sim.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of pspiceev.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 3ms 0 
.PROBE 
.INC "gerilimbolucu-SCHEMATIC1.net" 


**** INCLUDING gerilimbolucu-SCHEMATIC1.net ****
* source GERILIMBOLUCU
R_R1         N00009 N00015  1k  
R_R2         N00015 0  1k  
V_V1         N00009 0  
+SIN 0 10 1k 0 0 0

**** RESUMING gerilimbolucu-SCHEMATIC1-sim.sim.cir ****
.INC "gerilimbolucu-SCHEMATIC1.als"



**** INCLUDING gerilimbolucu-SCHEMATIC1.als ****
.ALIASES
R_R1            R1(1=N00009 2=N00015 )
R_R2            R2(1=N00015 2=0 )
V_V1            V1(+=N00009 -=0 )
.ENDALIASES

**** RESUMING gerilimbolucu-SCHEMATIC1-sim.sim.cir ****
.END

**** 02/15/10 16:26:33 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\gerilimbolucu\gerilimbolucu-SCHEMATIC1-sim.sim


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00009)    0.0000 (N00015)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1         0.000E+00

    TOTAL POWER DISSIPATION   0.00E+00  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .05
