
**** 02/15/10 16:59:15 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\diyot\diyot-SCHEMATIC1-sim.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "diyot-SCHEMATIC1-sim.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of pspiceev.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 0.06s 0 
.PROBE 
.INC "diyot-SCHEMATIC1.net" 


**** INCLUDING diyot-SCHEMATIC1.net ****
* source DIYOT
V_V1         N00011 0  
+SIN 0 12 50 0 0 0
C_C1         0 N00017  10u  
R_R1         0 N00017  1k  
D_D1         N00011 N00017 D1N4002 

**** RESUMING diyot-SCHEMATIC1-sim.sim.cir ****
.INC "diyot-SCHEMATIC1.als"



**** INCLUDING diyot-SCHEMATIC1.als ****
.ALIASES
V_V1            V1(+=N00011 -=0 )
C_C1            C1(1=0 2=N00017 )
R_R1            R1(1=0 2=N00017 )
D_D1            D1(1=N00011 2=N00017 )
.ENDALIASES

**** RESUMING diyot-SCHEMATIC1-sim.sim.cir ****
.END

**** 02/15/10 16:59:15 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\diyot\diyot-SCHEMATIC1-sim.sim ] 


 ****     Diode MODEL PARAMETERS


******************************************************************************




               D1N4002         
          IS   14.110000E-09 
           N    1.984        
         ISR  100.000000E-12 
         IKF   94.81         
          BV  100.1          
         IBV   10            
          RS     .03389      
          TT    4.761000E-06 
         CJO   51.170000E-12 
          VJ     .3905       
           M     .2762       


**** 02/15/10 16:59:15 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\diyot\diyot-SCHEMATIC1-sim.sim ] 


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00011)    0.0000 (N00017)-30.71E-21 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1         3.071E-23

    TOTAL POWER DISSIPATION   0.00E+00  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .11
