
**** 02/15/10 17:09:11 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\transistorACanaliz\transistoracanaliz-SCHEMATI


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "transistoracanaliz-SCHEMATIC1-sim.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of pspiceev.ini file:
.lib "nom.lib" 

*Analysis directives: 
.AC DEC 20 1 100MEG
.PROBE 
.INC "transistoracanaliz-SCHEMATIC1.net" 


**** INCLUDING transistoracanaliz-SCHEMATIC1.net ****
* source TRANSISTORACANALIZ
V_V1         N00056 0 12Vdc
C_C1         N00129 N00023  10u  
C_C2         N00046 N00059  10u  
C_C3         0 N00039  10u  
R_R1         N00023 N00056  100k  
R_R2         0 N00023  10k  
R_R3         0 N00039  270  
R_R4         N00046 N00056  2k  
R_R5         0 N00059  10k  
Q_Q1         N00046 N00023 N00039 Q2N2222
V_V2         N00129 0 DC 0Vdc AC 1Vac 

**** RESUMING transistoracanaliz-SCHEMATIC1-sim.sim.cir ****
.INC "transistoracanaliz-SCHEMATIC1.als"



**** INCLUDING transistoracanaliz-SCHEMATIC1.als ****
.ALIASES
V_V1            V1(+=N00056 -=0 )
C_C1            C1(1=N00129 2=N00023 )
C_C2            C2(1=N00046 2=N00059 )
C_C3            C3(1=0 2=N00039 )
R_R1            R1(1=N00023 2=N00056 )
R_R2            R2(1=0 2=N00023 )
R_R3            R3(1=0 2=N00039 )
R_R4            R4(1=N00046 2=N00056 )
R_R5            R5(1=0 2=N00059 )
Q_Q1            Q1(c=N00046 b=N00023 e=N00039 )
V_V2            V2(+=N00129 -=0 )
.ENDALIASES

**** RESUMING transistoracanaliz-SCHEMATIC1-sim.sim.cir ****
.END

**** 02/15/10 17:09:11 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\transistorACanaliz\transistoracanaliz-SCHEMATI


 ****     BJT MODEL PARAMETERS


******************************************************************************




               Q2N2222         
               NPN             
          IS   14.340000E-15 
          BF  255.9          
          NF    1            
         VAF   74.03         
         IKF     .2847       
         ISE   14.340000E-15 
          NE    1.307        
          BR    6.092        
          NR    1            
          RB   10            
          RC    1            
         CJE   22.010000E-12 
         MJE     .377        
         CJC    7.306000E-12 
         MJC     .3416       
          TF  411.100000E-12 
         XTF    3            
         VTF    1.7          
         ITF     .6          
          TR   46.910000E-09 
         XTB    1.5          
          CN    2.42         
           D     .87         


**** 02/15/10 17:09:11 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\transistorACanaliz\transistoracanaliz-SCHEMATI


 ****     SMALL SIGNAL BIAS SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00023)    1.0176 (N00039)     .3666 (N00046)    9.3006 (N00056)   12.0000     

(N00059)    0.0000 (N00129)    0.0000 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1        -1.460E-03
    V_V2         0.000E+00

    TOTAL POWER DISSIPATION   1.75E-02  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .08
