
**** 02/15/10 17:03:54 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\transistorDCanaliz\transistordcanaliz-SCHEMATI


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "transistordcanaliz-SCHEMATIC1-sim.sim.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Local Libraries :
* From [PSPICE NETLIST] section of pspiceev.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 1000ns 0 
.PROBE 
.INC "transistordcanaliz-SCHEMATIC1.net" 


**** INCLUDING transistordcanaliz-SCHEMATIC1.net ****
* source TRANSISTORDCANALIZ
Q_Q1         N00021 N00015 N00024 Q2N2222
R_R1         N00021 N00018  2k  
R_R2         0 N00024  270  
R_R3         N00018 N00015  100k  
R_R4         N00015 0  10k  
V_V1         N00018 0 12Vdc

**** RESUMING transistordcanaliz-SCHEMATIC1-sim.sim.cir ****
.INC "transistordcanaliz-SCHEMATIC1.als"



**** INCLUDING transistordcanaliz-SCHEMATIC1.als ****
.ALIASES
Q_Q1            Q1(c=N00021 b=N00015 e=N00024 )
R_R1            R1(1=N00021 2=N00018 )
R_R2            R2(1=0 2=N00024 )
R_R3            R3(1=N00018 2=N00015 )
R_R4            R4(1=N00015 2=0 )
V_V1            V1(+=N00018 -=0 )
.ENDALIASES

**** RESUMING transistordcanaliz-SCHEMATIC1-sim.sim.cir ****
.END

**** 02/15/10 17:03:54 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\transistorDCanaliz\transistordcanaliz-SCHEMATI


 ****     BJT MODEL PARAMETERS


******************************************************************************




               Q2N2222         
               NPN             
          IS   14.340000E-15 
          BF  255.9          
          NF    1            
         VAF   74.03         
         IKF     .2847       
         ISE   14.340000E-15 
          NE    1.307        
          BR    6.092        
          NR    1            
          RB   10            
          RC    1            
         CJE   22.010000E-12 
         MJE     .377        
         CJC    7.306000E-12 
         MJC     .3416       
          TF  411.100000E-12 
         XTF    3            
         VTF    1.7          
         ITF     .6          
          TR   46.910000E-09 
         XTB    1.5          
          CN    2.42         
           D     .87         


**** 02/15/10 17:03:54 *********** Evaluation PSpice (Nov 1999) **************

 ** Profile: "SCHEMATIC1-sim"  [ C:\Documents and Settings\acer\Belgelerim\pspiceogren\transistorDCanaliz\transistordcanaliz-SCHEMATI


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(N00015)    1.0176 (N00018)   12.0000 (N00021)    9.3006 (N00024)     .3666 




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1        -1.460E-03

    TOTAL POWER DISSIPATION   1.75E-02  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME             .03
